<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="3" y1="0" x2="157" y2="0" width="0" layer="20"/>
<wire x1="157" y1="0" x2="160" y2="3" width="0" layer="20" curve="90"/>
<wire x1="160" y1="3" x2="160" y2="47" width="0" layer="20"/>
<wire x1="160" y1="47" x2="157" y2="50" width="0" layer="20" curve="90"/>
<wire x1="157" y1="50" x2="89.8" y2="50" width="0" layer="20"/>
<wire x1="78.7" y1="50" x2="60.9" y2="50" width="0" layer="20"/>
<wire x1="59.9" y1="49.2" x2="51.5" y2="49.2" width="0" layer="20"/>
<wire x1="50.5" y1="50" x2="3" y2="50" width="0" layer="20"/>
<wire x1="3" y1="50" x2="0" y2="47" width="0" layer="20" curve="90"/>
<wire x1="0" y1="47" x2="0" y2="3" width="0" layer="20"/>
<wire x1="0" y1="3" x2="3" y2="0" width="0" layer="20" curve="90"/>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>OUT</text>
<text>IN</text>
<text>OUT</text>
<text>IN</text>
<wire x1="51.5" y1="49.2" x2="50.5" y2="50" width="0" layer="20" curve="-78.690068"/>
<wire x1="59.9" y1="49.2" x2="60.9" y2="50" width="0" layer="20" curve="78.690068"/>
<wire x1="78.7" y1="50" x2="79.7" y2="49" width="0" layer="20" curve="90"/>
<wire x1="79.7" y1="49" x2="88.8" y2="49" width="0" layer="20"/>
<wire x1="88.8" y1="49" x2="89.8" y2="50" width="0" layer="20" curve="90"/>
<wire x1="49" y1="8" x2="49" y2="0" width="2" layer="46"/>
<wire x1="49" y1="50" x2="49" y2="45" width="2" layer="46"/>
<wire x1="49" y1="35" x2="49" y2="29" width="2" layer="46"/>
<text>VDD</text>
<text>PB6</text>
<text>PB7</text>
<text>PB8</text>
<text>PB9</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>VDD</text>
<text>PC0</text>
<text>PC1</text>
<text>PC2</text>
<text>PC3</text>
<text>PC4</text>
<text>PC5</text>
<text>VDDA</text>
<text>PA0</text>
<text>PA1</text>
<text>PA2</text>
<text>PA3</text>
<text>VDDA</text>
<text>PA4</text>
<text>PA5</text>
<text>PA6</text>
<text>PA7</text>
<text>PB0</text>
<text>PB1</text>
<text>LED1</text>
<text>LED2</text>
<text>S1</text>
<text>S2</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>LIN+</text>
<text>LIN-</text>
<text>RIN-</text>
<text>RIN+</text>
<text>CM</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>VDDC</text>
<text>VDDC</text>
<text>R</text>
<text>T</text>
<text>S</text>
<text>S</text>
<text>S</text>
<text>T</text>
<text>T</text>
<text>R</text>
<text>R</text>
<text>ROUT+-</text>
<text>LOUT+-</text>
<text>GND</text>
<text>Axoloti Core 
  board outline
  connector/pad locations
  </text>
<text>v1.1 only!</text>
</plain>
<libraries>
<library name="con-hirschmann">
<description>&lt;b&gt;Hirschmann Connectors&lt;/b&gt;&lt;p&gt;
Audio, scart, microphone, headphone&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MAB5SH">
<description>Female &lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
5 pins 90 deg. with shield, horizontal (DIN 41524)</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="con-jack63">
<packages>
<package name="JACK63">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="axohw">
<packages>
<package name="PROTOHOLE_NAMED">
</package>
<package name="PROTOHOLE">
</package>
<package name="MOLEX_502774">
</package>
</packages>
</library>
<library name="switchcraft_smdminijackf">
<packages>
<package name="35RASMT4BHNTR">
</package>
</packages>
</library>
<library name="OLIMEX_CONNECTORS">
<packages>
<package name="USB_A_VERTICAL_PTH">
</package>
</packages>
</library>
<library name="switch_evqp7">
<packages>
<package name="EVQP7">
</package>
</packages>
</library>
<library name="led-sml-a12">
<packages>
<package name="SML-A12">
</package>
</packages>
</library>
<library name="j_usb_hirose_zx62d-b-5p8">
<packages>
<package name="ZX62D-B-5P8">
<description>Mounting pattern for Hirose ZX62D-B-5P8 Micro-B USB connector with SMD leads and through-hole shell connection. Modified from the manufacturer's recommendations by using round holes and leaving out shell SMD pads.</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2051">
<description>.100" (2.54mm) Center Header - 5 Pin</description>
</package>
<package name="22-23-2071">
<description>.100" (2.54mm) Center Header - 7 Pin</description>
</package>
<package name="22-23-2021">
<description>.100" (2.54mm) Center Headers - 2 Pin</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="PJ-102A">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X12" library="con-hirschmann" package="MAB5SH" value="MAB5SH">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="809883"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="CP-2350-ND"/>
<attribute name="PAGE" value="TH"/>
</element>
<element name="X13" library="con-hirschmann" package="MAB5SH" value="MAB5SH">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="809883"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="CP-2350-ND"/>
<attribute name="PAGE" value="TH"/>
</element>
<element name="H1" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H2" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H3" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H4" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="X7" library="con-jack63" package="JACK63" value=" NMJ6HFD2">
<attribute name="PAGE" value="TH"/>
</element>
<element name="X6" library="con-jack63" package="JACK63" value=" NMJ6HFD2">
<attribute name="PAGE" value="TH"/>
</element>
<element name="H5" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H6" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="TP61" library="axohw" package="PROTOHOLE_NAMED" value="GND">
<attribute name="VALUE"/>
</element>
<element name="TP44" library="axohw" package="PROTOHOLE_NAMED" value="PA7">
<attribute name="VALUE"/>
</element>
<element name="TP43" library="axohw" package="PROTOHOLE_NAMED" value="PA6">
<attribute name="VALUE"/>
</element>
<element name="TP42" library="axohw" package="PROTOHOLE_NAMED" value="PA5">
<attribute name="VALUE"/>
</element>
<element name="TP41" library="axohw" package="PROTOHOLE_NAMED" value="PA4">
<attribute name="VALUE"/>
</element>
<element name="TP40" library="axohw" package="PROTOHOLE_NAMED" value="PA3">
<attribute name="VALUE"/>
</element>
<element name="TP39" library="axohw" package="PROTOHOLE_NAMED" value="PA2">
<attribute name="VALUE"/>
</element>
<element name="TP38" library="axohw" package="PROTOHOLE_NAMED" value="PA1">
<attribute name="VALUE"/>
</element>
<element name="TP37" library="axohw" package="PROTOHOLE_NAMED" value="PA0">
<attribute name="VALUE"/>
</element>
<element name="TP60" library="axohw" package="PROTOHOLE_NAMED" value="GND">
<attribute name="VALUE"/>
</element>
<element name="TP46" library="axohw" package="PROTOHOLE_NAMED" value="PB1">
<attribute name="VALUE"/>
</element>
<element name="TP45" library="axohw" package="PROTOHOLE_NAMED" value="PB0">
<attribute name="VALUE"/>
</element>
<element name="TP56" library="axohw" package="PROTOHOLE_NAMED" value="PC5">
<attribute name="VALUE"/>
</element>
<element name="TP55" library="axohw" package="PROTOHOLE_NAMED" value="PC4">
<attribute name="VALUE"/>
</element>
<element name="TP62" library="axohw" package="PROTOHOLE_NAMED" value="GND">
<attribute name="VALUE"/>
</element>
<element name="TP51" library="axohw" package="PROTOHOLE_NAMED" value="PC0">
<attribute name="VALUE"/>
</element>
<element name="TP52" library="axohw" package="PROTOHOLE_NAMED" value="PC1">
<attribute name="VALUE"/>
</element>
<element name="TP53" library="axohw" package="PROTOHOLE_NAMED" value="PC2">
<attribute name="VALUE"/>
</element>
<element name="TP54" library="axohw" package="PROTOHOLE_NAMED" value="PC3">
<attribute name="VALUE"/>
</element>
<element name="TP50" library="axohw" package="PROTOHOLE_NAMED" value="PB9">
<attribute name="VALUE"/>
</element>
<element name="TP49" library="axohw" package="PROTOHOLE_NAMED" value="PB8">
<attribute name="VALUE"/>
</element>
<element name="TP47" library="axohw" package="PROTOHOLE_NAMED" value="PB6">
<attribute name="VALUE"/>
</element>
<element name="TP48" library="axohw" package="PROTOHOLE_NAMED" value="PB7">
<attribute name="VALUE"/>
</element>
<element name="TP64" library="axohw" package="PROTOHOLE_NAMED" value="VDD">
<attribute name="VALUE"/>
</element>
<element name="TP13" library="axohw" package="PROTOHOLE_NAMED" value="GND">
<attribute name="VALUE"/>
</element>
<element name="TP7" library="axohw" package="PROTOHOLE_NAMED" value="G">
<attribute name="VALUE"/>
</element>
<element name="TP4" library="axohw" package="PROTOHOLE_NAMED" value="CM">
<attribute name="VALUE"/>
</element>
<element name="TP1" library="axohw" package="PROTOHOLE_NAMED" value="VDDC">
<attribute name="VALUE"/>
</element>
<element name="TP65" library="axohw" package="PROTOHOLE_NAMED" value="VDD">
<attribute name="VALUE"/>
</element>
<element name="TP68" library="axohw" package="PROTOHOLE_NAMED" value="+5V">
<attribute name="VALUE"/>
</element>
<element name="TP69" library="axohw" package="PROTOHOLE_NAMED" value="+5V">
<attribute name="VALUE"/>
</element>
<element name="TP63" library="axohw" package="PROTOHOLE_NAMED" value="G">
<attribute name="VALUE"/>
</element>
<element name="TP58" library="axohw" package="PROTOHOLE_NAMED" value="GND">
<attribute name="VALUE"/>
</element>
<element name="TP59" library="axohw" package="PROTOHOLE_NAMED" value="G">
<attribute name="VALUE"/>
</element>
<element name="TP57" library="axohw" package="PROTOHOLE_NAMED" value="GND">
<attribute name="VALUE"/>
</element>
<element name="X11" library="axohw" package="MOLEX_502774" value="MOLEX_502774">
<attribute name="VALUE"/>
<attribute name="PAGE" value="TJ-0008"/>
</element>
<element name="TP70" library="axohw" package="PROTOHOLE_NAMED" value="+5V">
<attribute name="VALUE"/>
</element>
<element name="X9" library="switchcraft_smdminijackf" package="35RASMT4BHNTR" value="35RASMT4">
<attribute name="PAGE" value="TJ-0006"/>
</element>
<element name="TP19" library="axohw" package="PROTOHOLE" value=""/>
<element name="TP21" library="axohw" package="PROTOHOLE" value=""/>
<element name="TP23" library="axohw" package="PROTOHOLE" value=""/>
<element name="TP30" library="axohw" package="PROTOHOLE" value=""/>
<element name="TP28" library="axohw" package="PROTOHOLE" value=""/>
<element name="TP26" library="axohw" package="PROTOHOLE" value=""/>
<element name="TP31" library="axohw" package="PROTOHOLE" value="T"/>
<element name="TP33" library="axohw" package="PROTOHOLE" value="R"/>
<element name="TP35" library="axohw" package="PROTOHOLE" value="S"/>
<element name="USB1" library="OLIMEX_CONNECTORS" package="USB_A_VERTICAL_PTH" value="FCI 73725-0110BLF">
<attribute name="VALUE"/>
<attribute name="PAGE" value="TH"/>
</element>
<element name="S1" library="switch_evqp7" package="EVQP7" value="EVQP7">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="CKN10514TR-ND"/>
<attribute name="PAGE" value="TJ-0003"/>
</element>
<element name="S2" library="switch_evqp7" package="EVQP7" value="EVQP7">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="CKN10514TR-ND"/>
<attribute name="PAGE" value="TJ-0003"/>
</element>
<element name="H7" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="D5" library="led-sml-a12" package="SML-A12" value="SML-A12 RED">
<attribute name="DIGIKEY" value="160-1479-6-ND"/>
<attribute name="PAGE" value="TJ-0009?"/>
<attribute name="PAGE_NOTE" value="SAME FOOTPRINT AS TJ-0000"/>
</element>
<element name="D6" library="led-sml-a12" package="SML-A12" value="SML-A12 GREEN">
<attribute name="DIGIKEY" value="160-1478-6-ND"/>
<attribute name="PAGE" value="TJ-0000"/>
</element>
<element name="X10" library="j_usb_hirose_zx62d-b-5p8" package="ZX62D-B-5P8" value="ZX62D-B-5P8">
<attribute name="VALUE"/>
<attribute name="PAGE" value="TJ-0007"/>
</element>
<element name="JP1" library="pinhead" package="1X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H8" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="X4" library="con-molex" package="22-23-2051" value="NC (22-23-2051)">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="con-molex" package="22-23-2071" value="22-23-2071">
<attribute name="OC_NEWARK" value="56H0445"/>
<attribute name="MPN" value="22-23-2071"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1654534"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP71" library="axohw" package="PROTOHOLE_NAMED" value="VDDA">
<attribute name="VALUE"/>
</element>
<element name="TP72" library="axohw" package="PROTOHOLE_NAMED" value="VDDA">
<attribute name="VALUE"/>
</element>
<element name="TP14" library="axohw" package="PROTOHOLE_NAMED" value="SD1">
<attribute name="VALUE"/>
</element>
<element name="TP15" library="axohw" package="PROTOHOLE_NAMED" value="SD2">
<attribute name="VALUE"/>
</element>
<element name="TP16" library="axohw" package="PROTOHOLE_NAMED" value="VDD">
<attribute name="VALUE"/>
</element>
<element name="TP17" library="axohw" package="PROTOHOLE_NAMED" value="SDA">
<attribute name="VALUE"/>
</element>
<element name="TP18" library="axohw" package="PROTOHOLE_NAMED" value="SCL">
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP32" library="axohw" package="PROTOHOLE_NAMED" value="T">
<attribute name="VALUE"/>
</element>
<element name="TP34" library="axohw" package="PROTOHOLE_NAMED" value="R">
<attribute name="VALUE"/>
</element>
<element name="TP36" library="axohw" package="PROTOHOLE_NAMED" value="S">
<attribute name="VALUE"/>
</element>
<element name="TP24" library="axohw" package="PROTOHOLE_NAMED" value="T">
<attribute name="VALUE"/>
</element>
<element name="TP27" library="axohw" package="PROTOHOLE_NAMED" value="R">
<attribute name="VALUE"/>
</element>
<element name="TP29" library="axohw" package="PROTOHOLE_NAMED" value="S">
<attribute name="VALUE"/>
</element>
<element name="TP22" library="axohw" package="PROTOHOLE_NAMED" value="R">
<attribute name="VALUE"/>
</element>
<element name="TP20" library="axohw" package="PROTOHOLE_NAMED" value="S">
<attribute name="VALUE"/>
</element>
<element name="TP25" library="axohw" package="PROTOHOLE_NAMED" value="T">
<attribute name="VALUE"/>
</element>
<element name="X8" library="switchcraft_smdminijackf" package="35RASMT4BHNTR" value="NC (35RASMT4)">
<attribute name="PAGE" value="NC"/>
</element>
<element name="X5" library="switchcraft_smdminijackf" package="35RASMT4BHNTR" value="NC (35RASMT4)">
<attribute name="PAGE" value="NC"/>
</element>
<element name="TP2" library="axohw" package="PROTOHOLE_NAMED" value="MI3">
<attribute name="VALUE"/>
</element>
<element name="TP3" library="axohw" package="PROTOHOLE_NAMED" value="MI5">
<attribute name="VALUE"/>
</element>
<element name="TP5" library="axohw" package="PROTOHOLE_NAMED" value="MI1">
<attribute name="VALUE"/>
</element>
<element name="TP6" library="axohw" package="PROTOHOLE_NAMED" value="MI4">
<attribute name="VALUE"/>
</element>
<element name="TP8" library="axohw" package="PROTOHOLE_NAMED" value="MI2">
<attribute name="VALUE"/>
</element>
<element name="TP9" library="axohw" package="PROTOHOLE_NAMED" value="MIG">
<attribute name="VALUE"/>
</element>
<element name="TP10" library="axohw" package="PROTOHOLE_NAMED" value="MO3">
<attribute name="VALUE"/>
</element>
<element name="TP11" library="axohw" package="PROTOHOLE_NAMED" value="MO1">
<attribute name="VALUE"/>
</element>
<element name="TP12" library="axohw" package="PROTOHOLE_NAMED" value="MO5">
<attribute name="VALUE"/>
</element>
<element name="TP73" library="axohw" package="PROTOHOLE_NAMED" value="MO4">
<attribute name="VALUE"/>
</element>
<element name="TP74" library="axohw" package="PROTOHOLE_NAMED" value="MO2">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X05" value="NC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X05" value="NC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP75" library="axohw" package="PROTOHOLE_NAMED" value="LIN+"/>
<element name="TP78" library="axohw" package="PROTOHOLE_NAMED" value="LIN-"/>
<element name="TP79" library="axohw" package="PROTOHOLE_NAMED" value="RIN+"/>
<element name="TP80" library="axohw" package="PROTOHOLE_NAMED" value="RIN-"/>
<element name="TP66" library="axohw" package="PROTOHOLE_NAMED" value="VDDC"/>
<element name="TP67" library="axohw" package="PROTOHOLE_NAMED" value="G"/>
<element name="TP76" library="axohw" package="PROTOHOLE_NAMED" value="+5V"/>
<element name="X1" library="adafruit" package="PJ-102A" value="2.1MMJACKTHM">
<attribute name="FARNELL" value="1737246???"/>
<attribute name="PAGE" value="TH"/>
</element>
<element name="TP77" library="axohw" package="PROTOHOLE_NAMED" value="VDDC">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="NC">
</signal>
<signal name="VDD">
<contactref element="TP64" pad="P$1"/>
<contactref element="TP65" pad="P$1"/>
<contactref element="S1" pad="P$2"/>
<contactref element="S2" pad="P$2"/>
<contactref element="JP1" pad="1"/>
<contactref element="TP16" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="X13" pad="2"/>
<contactref element="X13" pad="PE@"/>
<contactref element="X13" pad="PE"/>
<contactref element="TP61" pad="P$1"/>
<contactref element="TP62" pad="P$1"/>
<contactref element="TP60" pad="P$1"/>
<contactref element="TP13" pad="P$1"/>
<contactref element="TP7" pad="P$1"/>
<contactref element="TP63" pad="P$1"/>
<contactref element="TP58" pad="P$1"/>
<contactref element="TP59" pad="P$1"/>
<contactref element="TP57" pad="P$1"/>
<contactref element="JP1" pad="3"/>
<contactref element="X4" pad="1"/>
<contactref element="X3" pad="1"/>
<contactref element="X2" pad="1"/>
<contactref element="TP74" pad="P$1"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP3" pad="5"/>
<contactref element="TP67" pad="P$1"/>
<contactref element="X1" pad="RING"/>
</signal>
<signal name="MIDIIN4">
<contactref element="X12" pad="4"/>
<contactref element="TP6" pad="P$1"/>
</signal>
<signal name="BLINN">
<contactref element="X6" pad="T"/>
<contactref element="TP26" pad="P$1"/>
<contactref element="TP24" pad="P$1"/>
<contactref element="X5" pad="P3"/>
</signal>
<signal name="BRINN">
<contactref element="X6" pad="R"/>
<contactref element="TP28" pad="P$1"/>
<contactref element="TP27" pad="P$1"/>
<contactref element="X5" pad="P2"/>
</signal>
<signal name="MIDIIN5">
<contactref element="X12" pad="5"/>
<contactref element="TP3" pad="P$1"/>
</signal>
<signal name="MIDIOUT4">
<contactref element="X13" pad="4"/>
<contactref element="TP73" pad="P$1"/>
</signal>
<signal name="+5V">
<contactref element="TP68" pad="P$1"/>
<contactref element="TP69" pad="P$1"/>
<contactref element="TP70" pad="P$1"/>
<contactref element="X3" pad="3"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="TP76" pad="P$1"/>
</signal>
<signal name="MIDIOUT5">
<contactref element="X13" pad="5"/>
<contactref element="TP12" pad="P$1"/>
</signal>
<signal name="N$73">
</signal>
<signal name="N$79">
</signal>
<signal name="N$98">
</signal>
<signal name="VDDC">
<contactref element="TP1" pad="P$1"/>
<contactref element="TP66" pad="P$1"/>
<contactref element="TP77" pad="P$1"/>
</signal>
<signal name="N$135">
</signal>
<signal name="BOOT0">
<contactref element="S1" pad="P$1"/>
</signal>
<signal name="PA0_GP">
<contactref element="TP37" pad="P$1"/>
</signal>
<signal name="PA1_GP">
<contactref element="TP38" pad="P$1"/>
</signal>
<signal name="PA2_GP">
<contactref element="TP39" pad="P$1"/>
</signal>
<signal name="PA3_GP">
<contactref element="TP40" pad="P$1"/>
</signal>
<signal name="PA4_GP">
<contactref element="TP41" pad="P$1"/>
</signal>
<signal name="PA5_GP">
<contactref element="TP42" pad="P$1"/>
</signal>
<signal name="PA6_GP">
<contactref element="TP43" pad="P$1"/>
</signal>
<signal name="PA7_GP">
<contactref element="TP44" pad="P$1"/>
</signal>
<signal name="PA13_SYS_JTMS_SWDIO">
<contactref element="JP1" pad="4"/>
</signal>
<signal name="PA14_SYS_JTMS_SWCLK">
<contactref element="JP1" pad="2"/>
</signal>
<signal name="!RST">
<contactref element="JP1" pad="5"/>
</signal>
<signal name="CM">
<contactref element="TP4" pad="P$1"/>
</signal>
<signal name="LOUTP">
</signal>
<signal name="LOUTN">
</signal>
<signal name="RHP">
<contactref element="X9" pad="P2"/>
<contactref element="TP23" pad="P$1"/>
<contactref element="TP25" pad="P$1"/>
</signal>
<signal name="LHP">
<contactref element="X9" pad="P3"/>
<contactref element="TP21" pad="P$1"/>
<contactref element="TP22" pad="P$1"/>
</signal>
<signal name="ROUTP">
</signal>
<signal name="ROUTN">
</signal>
<signal name="PB8_GP">
<contactref element="TP49" pad="P$1"/>
</signal>
<signal name="MONOOUT">
<contactref element="X9" pad="P1"/>
<contactref element="TP19" pad="P$1"/>
<contactref element="TP20" pad="P$1"/>
</signal>
<signal name="BLOUTP">
<contactref element="X7" pad="T"/>
<contactref element="TP31" pad="P$1"/>
<contactref element="TP32" pad="P$1"/>
<contactref element="X8" pad="P3"/>
</signal>
<signal name="BROUTP">
<contactref element="X7" pad="R"/>
<contactref element="TP33" pad="P$1"/>
<contactref element="TP34" pad="P$1"/>
<contactref element="X8" pad="P2"/>
</signal>
<signal name="PB1_GP">
<contactref element="TP46" pad="P$1"/>
</signal>
<signal name="PB0_GP">
<contactref element="TP45" pad="P$1"/>
</signal>
<signal name="PC5_GP">
<contactref element="TP56" pad="P$1"/>
</signal>
<signal name="PC4_GP">
<contactref element="TP55" pad="P$1"/>
</signal>
<signal name="PC0_GP">
<contactref element="TP51" pad="P$1"/>
</signal>
<signal name="PC1_GP">
<contactref element="TP52" pad="P$1"/>
</signal>
<signal name="PC2_GP">
<contactref element="TP53" pad="P$1"/>
</signal>
<signal name="PC3_GP">
<contactref element="TP54" pad="P$1"/>
</signal>
<signal name="PG6L">
<contactref element="D6" pad="A"/>
</signal>
<signal name="PB9_GP">
<contactref element="TP50" pad="P$1"/>
</signal>
<signal name="HSHIELD">
<contactref element="USB1" pad="P$3"/>
<contactref element="USB1" pad="P$4"/>
</signal>
<signal name="PB6_GP">
<contactref element="TP47" pad="P$1"/>
</signal>
<signal name="PB7_GP">
<contactref element="TP48" pad="P$1"/>
</signal>
<signal name="PB10_USART3TX">
<contactref element="X4" pad="5"/>
<contactref element="X3" pad="2"/>
</signal>
<signal name="PD6_SPI3MOSI">
<contactref element="X3" pad="4"/>
</signal>
<signal name="PE3_SAI1_SD_B">
<contactref element="TP15" pad="P$1"/>
</signal>
<signal name="PE4_SAI1_FS_A">
<contactref element="X4" pad="4"/>
</signal>
<signal name="PE5_SAI1_SCK_A">
<contactref element="X4" pad="3"/>
</signal>
<signal name="PE6_SAI1_SD_A">
<contactref element="TP14" pad="P$1"/>
</signal>
<signal name="PG9_USART6RX">
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="PG14_USART6TX">
<contactref element="JP2" pad="4"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="PH7_I2C3SCL">
<contactref element="TP18" pad="P$1"/>
</signal>
<signal name="PA8_MCO1">
<contactref element="X4" pad="2"/>
</signal>
<signal name="PH8_I2C3SDA">
<contactref element="TP17" pad="P$1"/>
</signal>
<signal name="PB3_SPI3SCK">
<contactref element="X3" pad="5"/>
</signal>
<signal name="PB4_SPI3MISO">
<contactref element="X3" pad="7"/>
</signal>
<signal name="VDDA1">
<contactref element="TP71" pad="P$1"/>
<contactref element="TP72" pad="P$1"/>
</signal>
<signal name="PA15_SPI3NSS">
<contactref element="X3" pad="6"/>
</signal>
<signal name="N$12">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
<signal name="N$18">
</signal>
<signal name="N$20">
</signal>
<signal name="N$22">
</signal>
<signal name="N$23">
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="N$27">
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
<signal name="N$30">
</signal>
<signal name="N$31">
</signal>
<signal name="N$32">
</signal>
<signal name="N$33">
</signal>
<signal name="N$34">
</signal>
<signal name="N$35">
</signal>
<signal name="N$36">
</signal>
<signal name="N$37">
</signal>
<signal name="N$48">
</signal>
<signal name="N$51">
</signal>
<signal name="N$52">
</signal>
<signal name="N$54">
</signal>
<signal name="N$55">
</signal>
<signal name="N$56">
</signal>
<signal name="N$57">
</signal>
<signal name="N$58">
</signal>
<signal name="N$59">
</signal>
<signal name="N$60">
</signal>
<signal name="N$63">
</signal>
<signal name="N$64">
</signal>
<signal name="N$65">
</signal>
<signal name="N$67">
</signal>
<signal name="N$69">
</signal>
<signal name="N$70">
</signal>
<signal name="N$71">
</signal>
<signal name="N$72">
</signal>
<signal name="N$74">
</signal>
<signal name="N$75">
</signal>
<signal name="N$76">
</signal>
<signal name="N$77">
</signal>
<signal name="N$78">
</signal>
<signal name="N$80">
</signal>
<signal name="N$81">
</signal>
<signal name="N$82">
</signal>
<signal name="HP_DUMMY1">
<contactref element="X9" pad="P5"/>
</signal>
<signal name="HP_DUMMY2">
<contactref element="X9" pad="P4"/>
</signal>
<signal name="VBUSEND">
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="OUTSGND">
<contactref element="X7" pad="S"/>
<contactref element="TP35" pad="P$1"/>
<contactref element="TP36" pad="P$1"/>
<contactref element="X8" pad="P1"/>
</signal>
<signal name="INSGND">
<contactref element="X6" pad="S"/>
<contactref element="TP30" pad="P$1"/>
<contactref element="TP29" pad="P$1"/>
<contactref element="X5" pad="P1"/>
</signal>
<signal name="MI3">
<contactref element="TP2" pad="P$1"/>
<contactref element="X12" pad="3"/>
</signal>
<signal name="MI1">
<contactref element="X12" pad="1"/>
<contactref element="TP5" pad="P$1"/>
</signal>
<signal name="MI2">
<contactref element="X12" pad="2"/>
<contactref element="TP8" pad="P$1"/>
</signal>
<signal name="MIG">
<contactref element="X12" pad="PE@"/>
<contactref element="X12" pad="PE"/>
<contactref element="TP9" pad="P$1"/>
</signal>
<signal name="MO3">
<contactref element="TP10" pad="P$1"/>
<contactref element="X13" pad="3"/>
</signal>
<signal name="MO1">
<contactref element="X13" pad="1"/>
<contactref element="TP11" pad="P$1"/>
</signal>
<signal name="N$26">
</signal>
<signal name="LIN+">
<contactref element="TP75" pad="P$1"/>
<contactref element="TP79" pad="P$1"/>
</signal>
<signal name="LIN-">
<contactref element="TP78" pad="P$1"/>
</signal>
<signal name="VINJACK1">
<contactref element="X2" pad="2"/>
<contactref element="X1" pad="TIP"/>
</signal>
<signal name="N$38">
</signal>
<signal name="N$42">
</signal>
<signal name="N$43">
</signal>
<signal name="N$44">
</signal>
<signal name="N$45">
</signal>
<signal name="RIN-">
<contactref element="TP80" pad="P$1"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
